<!--This work is licensed under a Creative Commons Attribution-ShareAlike 4.0 International License (CC BY-SA) with Design Exception 1.0-->
<eagle version="7.1.0">
<drawing>
<library>
<packages>
<package name="SOIC127P599X175-8N">
</package>
</packages>
<symbols>
<symbol name="TL072ACD">
<pin name="1IN+" direction="in"/>
<pin name="1IN-" direction="in"/>
<pin name="2IN+" direction="in"/>
<pin name="2IN-" direction="in"/>
<pin name="VCC+" direction="pwr"/>
<pin name="VCC-" direction="pwr"/>
<pin name="1OUT" direction="out"/>
<pin name="2OUT" direction="out"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="TL072ACD" prefix="U">
<description> &lt;a href="https://pricing.snapeda.com/parts/TL072ACD/Texas%20Instruments/view-part?ref=eda"&gt;Check prices&lt;/a&gt;</description>
<gates>
<gate name="A" symbol="TL072ACD"/>
</gates>
<devices>
<device name="" package="SOIC127P599X175-8N">
<connects>
<connect gate="A" pin="1IN+" pad="3"/>
<connect gate="A" pin="1IN-" pad="2"/>
<connect gate="A" pin="1OUT" pad="1"/>
<connect gate="A" pin="2IN+" pad="5"/>
<connect gate="A" pin="2IN-" pad="6"/>
<connect gate="A" pin="2OUT" pad="7"/>
<connect gate="A" pin="VCC+" pad="8"/>
<connect gate="A" pin="VCC-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="Purchase-URL" value="https://pricing.snapeda.com/search/part/TL072ACD/?ref=eda"/>
<attribute name="Package" value="SOIC-8 Texas Instruments"/>
<attribute name="MF" value="Texas Instruments"/>
<attribute name="Availability" value="Good"/>
<attribute name="Description" value="
Dual low-noise JFET-input improved offset operational amplifier 8-SOIC 0 to 70
"/>
<attribute name="MP" value="TL072ACD"/>
<attribute name="Price" value="None"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
