(footprint "LED_SK6812_PLCC4_5.0x5.0mm_P3.2mm_ThroughPCB"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "5.0mm x 5.0mm Addressable RGB LED NeoPixel, https://cdn-shop.adafruit.com/product-files/1138/SK6812+LED+datasheet+.pdf")
	(tags "LED RGB NeoPixel PLCC-4 5050")
	(property "Reference" "REF**"
		(at 0 -0.75 180)
		(layer "B.SilkS")
		(uuid "eee40459-a8b8-4e85-ba09-4b05cce49d82")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
			(justify mirror)
		)
	)
	(property "Value" "LED_SK6812_PLCC4_5.0x5.0mm_P3.2mm_ThroughPCB"
		(at 0 6.75 0)
		(layer "F.Fab")
		(uuid "b950a9bb-c03d-4274-9319-17f8a0ab880e")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Datasheet" ""
		(at 0 2.75 180)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "201eb1bd-5c4e-4b39-95c3-3de574054db9")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "Description" ""
		(at 0 2.75 180)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "1bf8c2c0-c2f8-4320-9d19-2109fda1b53c")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(attr smd)
	(fp_line
		(start -3.5 0.45)
		(end -3.5 5.5)
		(stroke
			(width 0.12)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "e335b6dc-d57d-46e4-b673-56382037432b")
	)
	(fp_line
		(start -3.05 0)
		(end -3.5 0.45)
		(stroke
			(width 0.12)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "e2142307-77e2-4b73-8355-cf8a0a60214c")
	)
	(fp_line
		(start 3.5 0)
		(end -3.05 0)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "a6a776d1-33ab-429d-a453-f6ac328450e5")
	)
	(fp_line
		(start 3.5 5.5)
		(end -3.5 5.5)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "ca7c0f9b-63cb-43f0-9286-b16c8ca32039")
	)
	(fp_line
		(start 3.5 5.5)
		(end 3.5 0)
		(stroke
			(width 0.12)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "85ddbb95-16ac-4b0b-86da-ea2c5c0f5e1b")
	)
	(fp_line
		(start -3.5 0.45)
		(end -3.5 5.5)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "B.SilkS")
		(uuid "5d074e71-b8eb-41eb-8736-084260fa5439")
	)
	(fp_line
		(start -3.05 0)
		(end -3.5 0.45)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "B.SilkS")
		(uuid "da3814da-74d4-4220-ba8a-5e6dd5ae4289")
	)
	(fp_line
		(start -2.5 3.65)
		(end -2.5 1.85)
		(stroke
			(width 0.12)
			(type default)
		)
		(layer "B.SilkS")
		(uuid "5e6c71ba-92c0-4645-a477-c91cb4703d75")
	)
	(fp_line
		(start 2.7 3.65)
		(end 2.7 1.85)
		(stroke
			(width 0.12)
			(type default)
		)
		(layer "B.SilkS")
		(uuid "b0b4fdd9-c0c9-4c0c-b6e4-7b2326a7209f")
	)
	(fp_line
		(start 3.5 0)
		(end -3.05 0)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "B.SilkS")
		(uuid "f7936c39-a227-42d1-a5df-2c74ea6d6357")
	)
	(fp_line
		(start 3.5 5.5)
		(end -3.5 5.5)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "B.SilkS")
		(uuid "da941860-a35f-4238-b9e8-bacaea476490")
	)
	(fp_line
		(start 3.5 5.5)
		(end 3.5 0)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "B.SilkS")
		(uuid "cf1cf262-01de-4968-a3ab-ac1a00b76e67")
	)
	(fp_circle
		(center 0 2.75)
		(end 2 2.75)
		(stroke
			(width 0.05)
			(type solid)
		)
		(fill no)
		(layer "Edge.Cuts")
		(uuid "8bff868e-c739-47e5-a1fa-a13eebb35e00")
	)
	(fp_line
		(start -3.45 0)
		(end -3.45 5.5)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "eb4e5a9f-2dc8-45fb-be9a-d2fcb3ea9f59")
	)
	(fp_line
		(start -3.45 5.5)
		(end 3.45 5.5)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "97077d3f-8a3e-4ba6-b2ee-f57ffd365f6e")
	)
	(fp_line
		(start 3.45 0)
		(end -3.45 0)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "6b3223e6-7f3f-4de0-9a81-2f93a2f94f7c")
	)
	(fp_line
		(start 3.45 5.5)
		(end 3.45 0)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "0a5d758d-d23f-41c5-9784-e94c185415b9")
	)
	(fp_line
		(start -2.5 0.25)
		(end -2.5 5.25)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "f5a17e42-ab37-4a38-8094-f624ab6c6fe3")
	)
	(fp_line
		(start -2.5 1.25)
		(end -1.5 0.25)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "f22bd8a5-67a5-4d34-af47-872c8e996657")
	)
	(fp_line
		(start -2.5 5.25)
		(end 2.5 5.25)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "9e1199e2-3c1e-47e6-9163-78c1822a90eb")
	)
	(fp_line
		(start 2.5 0.25)
		(end -2.5 0.25)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "83a65986-cc1c-4767-a1b8-c1c7bfeec89e")
	)
	(fp_line
		(start 2.5 5.25)
		(end 2.5 0.25)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "7ce498f5-0014-4e67-9634-59bb617e9383")
	)
	(fp_circle
		(center 0 2.75)
		(end 0 4.75)
		(stroke
			(width 0.1)
			(type solid)
		)
		(fill no)
		(layer "F.Fab")
		(uuid "2b25c03d-f65a-4448-8d85-ff2ea8ad29ec")
	)
	(fp_text user "${REFERENCE}"
		(at 0 2.75 0)
		(layer "F.Fab")
		(uuid "384985e0-9d96-44d4-a517-d4b5551aea8c")
		(effects
			(font
				(size 0.8 0.8)
				(thickness 0.15)
			)
		)
	)
	(pad "1" smd rect
		(at -2.45 1.15 180)
		(size 1.5 1)
		(layers "B.Cu" "B.Mask" "B.Paste")
		(uuid "98c0776d-12ee-4925-979d-e6f185bef9ce")
	)
	(pad "2" smd rect
		(at -2.45 4.35 180)
		(size 1.5 1)
		(layers "B.Cu" "B.Mask" "B.Paste")
		(uuid "9f7c7f30-2e0e-4df5-af1d-1d3853e2776e")
	)
	(pad "3" smd rect
		(at 2.45 4.35 180)
		(size 1.5 1)
		(layers "B.Cu" "B.Mask" "B.Paste")
		(uuid "088f7fe1-40a9-4e05-8019-68bb65ef1a2c")
	)
	(pad "4" smd rect
		(at 2.45 1.15 180)
		(size 1.5 1)
		(layers "B.Cu" "B.Mask" "B.Paste")
		(uuid "fb2ff826-1449-44e4-95ed-947ecaa01cb9")
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/LED_SMD.3dshapes/LED_SK6812_PLCC4_5.0x5.0mm_P3.2mm.step"
		(offset
			(xyz 0 -2.75 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
