(footprint "LED_SK6812_ThroughPCB"
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(layer "F.Cu")
	(property "Reference" "LED1"
		(at 0 -0.5 0)
		(unlocked yes)
		(layer "F.SilkS")
		(hide yes)
		(uuid "62e636fc-0e8d-4079-afb8-74a26c28bf3b")
		(effects
			(font
				(size 1 1)
				(thickness 0.1)
			)
		)
	)
	(property "Value" "SK6812"
		(at 0 8 0)
		(unlocked yes)
		(layer "F.Fab")
		(uuid "0f5e9e6b-7695-479c-9a43-7da931850d3e")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Footprint" "Macropad_Custom:LED_SK6812_ThroughPCB"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "622481ac-17e0-4c28-9808-6a6337aef013")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Datasheet" "https://cdn-shop.adafruit.com/product-files/1138/SK6812+LED+datasheet+.pdf"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "b59fb31b-18a3-443f-a9c5-69eff0afecfe")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Description" "RGB LED with integrated controller"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "cabc5597-dcdd-4279-8f2c-c7d33315d35f")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(attr smd)
	(fp_line
		(start -3.5 0.5)
		(end -3.5 0.6)
		(stroke
			(width 0.12)
			(type default)
		)
		(layer "B.SilkS")
		(uuid "fd0e4e59-df10-443e-9209-1c93b251e7c9")
	)
	(fp_line
		(start -3.5 0.5)
		(end -3 0)
		(stroke
			(width 0.12)
			(type default)
		)
		(layer "B.SilkS")
		(uuid "ce9d935b-ff7c-4c28-b614-08f76da2b8ba")
	)
	(fp_line
		(start -3.5 3.8)
		(end -3.5 1.7)
		(stroke
			(width 0.12)
			(type default)
		)
		(layer "B.SilkS")
		(uuid "6be20469-4ef9-4e1d-9768-b55a41543ee1")
	)
	(fp_line
		(start -3.5 5.5)
		(end -3.5 4.9)
		(stroke
			(width 0.12)
			(type default)
		)
		(layer "B.SilkS")
		(uuid "e5ec3e26-9e66-45c1-a3b1-5d70a3618001")
	)
	(fp_line
		(start -3 0)
		(end 3.4 0)
		(stroke
			(width 0.12)
			(type default)
		)
		(layer "B.SilkS")
		(uuid "da54e6d1-4534-49be-8ab9-4be72d174845")
	)
	(fp_line
		(start 3.4 0)
		(end 3.4 0.6)
		(stroke
			(width 0.12)
			(type default)
		)
		(layer "B.SilkS")
		(uuid "87fc67ec-197e-4f66-9193-fd91114b4b61")
	)
	(fp_line
		(start 3.4 1.7)
		(end 3.4 3.8)
		(stroke
			(width 0.12)
			(type default)
		)
		(layer "B.SilkS")
		(uuid "0319ff98-73a0-4569-b403-41fbda4b6fed")
	)
	(fp_line
		(start 3.4 5.5)
		(end -3.5 5.5)
		(stroke
			(width 0.12)
			(type default)
		)
		(layer "B.SilkS")
		(uuid "ae13e571-36a9-4d2f-a944-d81a9c8521eb")
	)
	(fp_line
		(start 3.4 5.5)
		(end 3.4 4.9)
		(stroke
			(width 0.12)
			(type default)
		)
		(layer "B.SilkS")
		(uuid "3099245d-ce79-47f6-b340-a476871e3500")
	)
	(fp_line
		(start -3.5 0.5)
		(end -3.5 0.6)
		(stroke
			(width 0.12)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "1a2b3ae3-6efd-4197-95a9-8b4b29f43cb5")
	)
	(fp_line
		(start -3.5 3.8)
		(end -3.5 1.7)
		(stroke
			(width 0.12)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "83e0a369-2348-4b93-ae18-a174274adaa0")
	)
	(fp_line
		(start -3.5 5.5)
		(end -3.5 4.9)
		(stroke
			(width 0.12)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "8f604df6-5417-450d-a0b5-6cee3733ba84")
	)
	(fp_line
		(start -3 0)
		(end -3.5 0.5)
		(stroke
			(width 0.12)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "35021777-7f28-4bd6-b5fa-bcee02f66e15")
	)
	(fp_line
		(start -2.75 1.85)
		(end -2.75 3.65)
		(stroke
			(width 0.12)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "db4a72f7-1f4a-4d06-b478-8e7a5d4c1542")
	)
	(fp_line
		(start 2.65 1.85)
		(end 2.65 3.65)
		(stroke
			(width 0.12)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "1ad893f4-2d48-4d55-9f49-5fde4e5d3099")
	)
	(fp_line
		(start 3.4 0)
		(end -3 0)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "0bf97e32-251f-4e8a-a602-bed3a1ead697")
	)
	(fp_line
		(start 3.4 0.6)
		(end 3.4 0)
		(stroke
			(width 0.12)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "aaad31ac-a06b-4d38-a7ba-9011f4d2f134")
	)
	(fp_line
		(start 3.4 3.8)
		(end 3.4 1.7)
		(stroke
			(width 0.12)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "39b39616-8ca3-4f28-8f14-bf90badec1c3")
	)
	(fp_line
		(start 3.4 5.5)
		(end -3.5 5.5)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "d923f84e-552b-4334-aa9b-7312cd9f8c48")
	)
	(fp_line
		(start 3.4 5.5)
		(end 3.4 4.9)
		(stroke
			(width 0.12)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "f8a7d077-7d87-4bed-a04d-3193d5e00ece")
	)
	(fp_rect
		(start -2.6 0.2)
		(end 2.5 5.3)
		(stroke
			(width 0.05)
			(type default)
		)
		(fill none)
		(layer "Edge.Cuts")
		(uuid "15bf2854-73a1-4476-b57e-2c0d2f46af91")
	)
	(fp_line
		(start -3.5 0)
		(end -3.5 5.5)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "48c56347-1d4b-4203-b28b-d7fb2042b068")
	)
	(fp_line
		(start -3.5 5.5)
		(end 3.4 5.5)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "81b8dc9a-c172-4e27-859b-72c767023b0a")
	)
	(fp_line
		(start 3.4 0)
		(end -3.5 0)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "6cbd4e1d-9a85-413d-b3ee-e794cf9e4f67")
	)
	(fp_line
		(start 3.4 5.5)
		(end 3.4 0)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "450f5b43-bd4b-4c27-a92c-b65f7965a67a")
	)
	(fp_text user "${REFERENCE}"
		(at -0.05 2.75 0)
		(layer "F.Fab")
		(uuid "86f93340-8ef9-414b-baa0-9582afd0428d")
		(effects
			(font
				(size 0.8 0.8)
				(thickness 0.15)
			)
		)
	)
	(fp_text user "${REFERENCE}"
		(at 0 6.5 0)
		(unlocked yes)
		(layer "F.Fab")
		(uuid "de9115ea-4c72-447d-9a1e-9650beb7ed70")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(pad "1" smd rect
		(at -3.4 1.15 180)
		(size 1.5 1)
		(layers "B.Cu" "B.Paste" "B.Mask")
		(uuid "cd064e6f-5c8a-44b8-b8d8-11376edaae7b")
	)
	(pad "2" smd rect
		(at -3.4 4.35 180)
		(size 1.5 1)
		(layers "B.Cu" "B.Paste" "B.Mask")
		(uuid "8aec36d9-e0e9-449e-a984-641bb80a657f")
	)
	(pad "3" smd rect
		(at 3.3 4.35 180)
		(size 1.5 1)
		(layers "B.Cu" "B.Paste" "B.Mask")
		(uuid "3aa85a3f-6d8f-479b-a115-d4f9a1ccc5b2")
	)
	(pad "4" smd rect
		(at 3.3 1.15 180)
		(size 1.5 1)
		(layers "B.Cu" "B.Paste" "B.Mask")
		(uuid "68a8b607-ba59-4d23-a95e-5f59357681ec")
	)
)
