<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.6.2">
<drawing>
<board>
<plain>
<wire x1="0" y1="100" x2="0" y2="0" width="0" layer="20"/>
<wire x1="0" y1="0" x2="100" y2="0" width="0.0762" layer="20"/>
<wire x1="100" y1="0" x2="100" y2="100" width="0.0762" layer="20"/>
<wire x1="100" y1="100" x2="0" y2="100" width="0.0762" layer="20"/>
<text>ZOE - Simple Saw VCO</text>
<text>1000-2_SimpleSaw
PCB Revision 1.0
March 2021</text>
<text>Designed in Ontario, Canada</text>
</plain>
<libraries>
<library name="rcl">
<description>&lt;b&gt;Resistors, Capacitors, Inductors&lt;/b&gt;&lt;p&gt;
Based on the previous libraries:
&lt;ul&gt;
&lt;li&gt;r.lbr
&lt;li&gt;cap.lbr 
&lt;li&gt;cap-fe.lbr
&lt;li&gt;captant.lbr
&lt;li&gt;polcap.lbr
&lt;li&gt;ipc-smd.lbr
&lt;/ul&gt;
All SMD packages are defined according to the IPC specifications and  CECC&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;&lt;p&gt;
&lt;p&gt;
for Electrolyt Capacitors see also :&lt;p&gt;
www.bccomponents.com &lt;p&gt;
www.panasonic.com&lt;p&gt;
www.kemet.com&lt;p&gt;
http://www.secc.co.jp/pdf/os_e/2004/e_os_all.pdf &lt;b&gt;(SANYO)&lt;/b&gt;
&lt;p&gt;
for trimmer refence see : &lt;u&gt;www.electrospec-inc.com/cross_references/trimpotcrossref.asp&lt;/u&gt;&lt;p&gt;

&lt;table border=0 cellspacing=0 cellpadding=0 width="100%" cellpaddding=0&gt;
&lt;tr valign="top"&gt;

&lt;! &lt;td width="10"&gt;&amp;nbsp;&lt;/td&gt;
&lt;td width="90%"&gt;

&lt;b&gt;&lt;font color="#0000FF" size="4"&gt;TRIM-POT CROSS REFERENCE&lt;/font&gt;&lt;/b&gt;
&lt;P&gt;
&lt;TABLE BORDER=0 CELLSPACING=1 CELLPADDING=2&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=8&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;RECTANGULAR MULTI-TURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;BOURNS&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;BI&amp;nbsp;TECH&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;DALE-VISHAY&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;PHILIPS/MEPCO&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;MURATA&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;PANASONIC&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;SPECTROL&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;MILSPEC&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;&lt;TD&gt;&amp;nbsp;&lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3 &gt;
      3005P&lt;BR&gt;
      3006P&lt;BR&gt;
      3006W&lt;BR&gt;
      3006Y&lt;BR&gt;
      3009P&lt;BR&gt;
      3009W&lt;BR&gt;
      3009Y&lt;BR&gt;
      3057J&lt;BR&gt;
      3057L&lt;BR&gt;
      3057P&lt;BR&gt;
      3057Y&lt;BR&gt;
      3059J&lt;BR&gt;
      3059L&lt;BR&gt;
      3059P&lt;BR&gt;
      3059Y&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      89P&lt;BR&gt;
      89W&lt;BR&gt;
      89X&lt;BR&gt;
      89PH&lt;BR&gt;
      76P&lt;BR&gt;
      89XH&lt;BR&gt;
      78SLT&lt;BR&gt;
      78L&amp;nbsp;ALT&lt;BR&gt;
      56P&amp;nbsp;ALT&lt;BR&gt;
      78P&amp;nbsp;ALT&lt;BR&gt;
      T8S&lt;BR&gt;
      78L&lt;BR&gt;
      56P&lt;BR&gt;
      78P&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      T18/784&lt;BR&gt;
      783&lt;BR&gt;
      781&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      2199&lt;BR&gt;
      1697/1897&lt;BR&gt;
      1680/1880&lt;BR&gt;
      2187&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      8035EKP/CT20/RJ-20P&lt;BR&gt;
      -&lt;BR&gt;
      RJ-20X&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      1211L&lt;BR&gt;
      8012EKQ&amp;nbsp;ALT&lt;BR&gt;
      8012EKR&amp;nbsp;ALT&lt;BR&gt;
      1211P&lt;BR&gt;
      8012EKJ&lt;BR&gt;
      8012EKL&lt;BR&gt;
      8012EKQ&lt;BR&gt;
      8012EKR&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      2101P&lt;BR&gt;
      2101W&lt;BR&gt;
      2101Y&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      2102L&lt;BR&gt;
      2102S&lt;BR&gt;
      2102Y&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      EVMCOG&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      43P&lt;BR&gt;
      43W&lt;BR&gt;
      43Y&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      40L&lt;BR&gt;
      40P&lt;BR&gt;
      40Y&lt;BR&gt;
      70Y-T602&lt;BR&gt;
      70L&lt;BR&gt;
      70P&lt;BR&gt;
      70Y&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      RT/RTR12&lt;BR&gt;
      RT/RTR12&lt;BR&gt;
      RT/RTR12&lt;BR&gt;
      -&lt;BR&gt;
      RJ/RJR12&lt;BR&gt;
      RJ/RJR12&lt;BR&gt;
      RJ/RJR12&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=8&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=8&gt;
      &lt;FONT SIZE=4 FACE=ARIAL&gt;&lt;B&gt;SQUARE MULTI-TURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
   &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BOURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BI&amp;nbsp;TECH&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;DALE-VISHAY&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PHILIPS/MEPCO&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;MURATA&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PANASONIC&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;SPECTROL&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;MILSPEC&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      3250L&lt;BR&gt;
      3250P&lt;BR&gt;
      3250W&lt;BR&gt;
      3250X&lt;BR&gt;
      3252P&lt;BR&gt;
      3252W&lt;BR&gt;
      3252X&lt;BR&gt;
      3260P&lt;BR&gt;
      3260W&lt;BR&gt;
      3260X&lt;BR&gt;
      3262P&lt;BR&gt;
      3262W&lt;BR&gt;
      3262X&lt;BR&gt;
      3266P&lt;BR&gt;
      3266W&lt;BR&gt;
      3266X&lt;BR&gt;
      3290H&lt;BR&gt;
      3290P&lt;BR&gt;
      3290W&lt;BR&gt;
      3292P&lt;BR&gt;
      3292W&lt;BR&gt;
      3292X&lt;BR&gt;
      3296P&lt;BR&gt;
      3296W&lt;BR&gt;
      3296X&lt;BR&gt;
      3296Y&lt;BR&gt;
      3296Z&lt;BR&gt;
      3299P&lt;BR&gt;
      3299W&lt;BR&gt;
      3299X&lt;BR&gt;
      3299Y&lt;BR&gt;
      3299Z&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      66P&amp;nbsp;ALT&lt;BR&gt;
      66W&amp;nbsp;ALT&lt;BR&gt;
      66X&amp;nbsp;ALT&lt;BR&gt;
      66P&amp;nbsp;ALT&lt;BR&gt;
      66W&amp;nbsp;ALT&lt;BR&gt;
      66X&amp;nbsp;ALT&lt;BR&gt;
      -&lt;BR&gt;
      64W&amp;nbsp;ALT&lt;BR&gt;
      -&lt;BR&gt;
      64P&amp;nbsp;ALT&lt;BR&gt;
      64W&amp;nbsp;ALT&lt;BR&gt;
      64X&amp;nbsp;ALT&lt;BR&gt;
      64P&lt;BR&gt;
      64W&lt;BR&gt;
      64X&lt;BR&gt;
      66X&amp;nbsp;ALT&lt;BR&gt;
      66P&amp;nbsp;ALT&lt;BR&gt;
      66W&amp;nbsp;ALT&lt;BR&gt;
      66P&lt;BR&gt;
      66W&lt;BR&gt;
      66X&lt;BR&gt;
      67P&lt;BR&gt;
      67W&lt;BR&gt;
      67X&lt;BR&gt;
      67Y&lt;BR&gt;
      67Z&lt;BR&gt;
      68P&lt;BR&gt;
      68W&lt;BR&gt;
      68X&lt;BR&gt;
      67Y&amp;nbsp;ALT&lt;BR&gt;
      67Z&amp;nbsp;ALT&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      5050&lt;BR&gt;
      5091&lt;BR&gt;
      5080&lt;BR&gt;
      5087&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      T63YB&lt;BR&gt;
      T63XB&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      5887&lt;BR&gt;
      5891&lt;BR&gt;
      5880&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      T93Z&lt;BR&gt;
      T93YA&lt;BR&gt;
      T93XA&lt;BR&gt;
      T93YB&lt;BR&gt;
      T93XB&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      8026EKP&lt;BR&gt;
      8026EKW&lt;BR&gt;
      8026EKM&lt;BR&gt;
      8026EKP&lt;BR&gt;
      8026EKB&lt;BR&gt;
      8026EKM&lt;BR&gt;
      1309X&lt;BR&gt;
      1309P&lt;BR&gt;
      1309W&lt;BR&gt;
      8024EKP&lt;BR&gt;
      8024EKW&lt;BR&gt;
      8024EKN&lt;BR&gt;
      RJ-9P/CT9P&lt;BR&gt;
      RJ-9W&lt;BR&gt;
      RJ-9X&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      3103P&lt;BR&gt;
      3103Y&lt;BR&gt;
      3103Z&lt;BR&gt;
      3103P&lt;BR&gt;
      3103Y&lt;BR&gt;
      3103Z&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      3105P/3106P&lt;BR&gt;
      3105W/3106W&lt;BR&gt;
      3105X/3106X&lt;BR&gt;
      3105Y/3106Y&lt;BR&gt;
      3105Z/3105Z&lt;BR&gt;
      3102P&lt;BR&gt;
      3102W&lt;BR&gt;
      3102X&lt;BR&gt;
      3102Y&lt;BR&gt;
      3102Z&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      EVMCBG&lt;BR&gt;
      EVMCCG&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      55-1-X&lt;BR&gt;
      55-4-X&lt;BR&gt;
      55-3-X&lt;BR&gt;
      55-2-X&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      50-2-X&lt;BR&gt;
      50-4-X&lt;BR&gt;
      50-3-X&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      64P&lt;BR&gt;
      64W&lt;BR&gt;
      64X&lt;BR&gt;
      64Y&lt;BR&gt;
      64Z&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      RT/RTR22&lt;BR&gt;
      RT/RTR22&lt;BR&gt;
      RT/RTR22&lt;BR&gt;
      RT/RTR22&lt;BR&gt;
      RJ/RJR22&lt;BR&gt;
      RJ/RJR22&lt;BR&gt;
      RJ/RJR22&lt;BR&gt;
      RT/RTR26&lt;BR&gt;
      RT/RTR26&lt;BR&gt;
      RT/RTR26&lt;BR&gt;
      RJ/RJR26&lt;BR&gt;
      RJ/RJR26&lt;BR&gt;
      RJ/RJR26&lt;BR&gt;
      RJ/RJR26&lt;BR&gt;
      RJ/RJR26&lt;BR&gt;
      RJ/RJR26&lt;BR&gt;
      RT/RTR24&lt;BR&gt;
      RT/RTR24&lt;BR&gt;
      RT/RTR24&lt;BR&gt;
      RJ/RJR24&lt;BR&gt;
      RJ/RJR24&lt;BR&gt;
      RJ/RJR24&lt;BR&gt;
      RJ/RJR24&lt;BR&gt;
      RJ/RJR24&lt;BR&gt;
      RJ/RJR24&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=8&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=8&gt;
      &lt;FONT SIZE=4 FACE=ARIAL&gt;&lt;B&gt;SINGLE TURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BOURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BI&amp;nbsp;TECH&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;DALE-VISHAY&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PHILIPS/MEPCO&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;MURATA&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PANASONIC&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;SPECTROL&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;MILSPEC&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      3323P&lt;BR&gt;
      3323S&lt;BR&gt;
      3323W&lt;BR&gt;
      3329H&lt;BR&gt;
      3329P&lt;BR&gt;
      3329W&lt;BR&gt;
      3339H&lt;BR&gt;
      3339P&lt;BR&gt;
      3339W&lt;BR&gt;
      3352E&lt;BR&gt;
      3352H&lt;BR&gt;
      3352K&lt;BR&gt;
      3352P&lt;BR&gt;
      3352T&lt;BR&gt;
      3352V&lt;BR&gt;
      3352W&lt;BR&gt;
      3362H&lt;BR&gt;
      3362M&lt;BR&gt;
      3362P&lt;BR&gt;
      3362R&lt;BR&gt;
      3362S&lt;BR&gt;
      3362U&lt;BR&gt;
      3362W&lt;BR&gt;
      3362X&lt;BR&gt;
      3386B&lt;BR&gt;
      3386C&lt;BR&gt;
      3386F&lt;BR&gt;
      3386H&lt;BR&gt;
      3386K&lt;BR&gt;
      3386M&lt;BR&gt;
      3386P&lt;BR&gt;
      3386S&lt;BR&gt;
      3386W&lt;BR&gt;
      3386X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      25P&lt;BR&gt;
      25S&lt;BR&gt;
      25RX&lt;BR&gt;
      82P&lt;BR&gt;
      82M&lt;BR&gt;
      82PA&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      91E&lt;BR&gt;
      91X&lt;BR&gt;
      91T&lt;BR&gt;
      91B&lt;BR&gt;
      91A&lt;BR&gt;
      91V&lt;BR&gt;
      91W&lt;BR&gt;
      25W&lt;BR&gt;
      25V&lt;BR&gt;
      25P&lt;BR&gt;
      -&lt;BR&gt;
      25S&lt;BR&gt;
      25U&lt;BR&gt;
      25RX&lt;BR&gt;
      25X&lt;BR&gt;
      72XW&lt;BR&gt;
      72XL&lt;BR&gt;
      72PM&lt;BR&gt;
      72RX&lt;BR&gt;
      -&lt;BR&gt;
      72PX&lt;BR&gt;
      72P&lt;BR&gt;
      72RXW&lt;BR&gt;
      72RXL&lt;BR&gt;
      72X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      T7YB&lt;BR&gt;
      T7YA&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      TXD&lt;BR&gt;
      TYA&lt;BR&gt;
      TYP&lt;BR&gt;
      -&lt;BR&gt;
      TYD&lt;BR&gt;
      TX&lt;BR&gt;
      -&lt;BR&gt;
      150SX&lt;BR&gt;
      100SX&lt;BR&gt;
      102T&lt;BR&gt;
      101S&lt;BR&gt;
      190T&lt;BR&gt;
      150TX&lt;BR&gt;
      101&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      101SX&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      ET6P&lt;BR&gt;
      ET6S&lt;BR&gt;
      ET6X&lt;BR&gt;
      RJ-6W/8014EMW&lt;BR&gt;
      RJ-6P/8014EMP&lt;BR&gt;
      RJ-6X/8014EMX&lt;BR&gt;
      TM7W&lt;BR&gt;
      TM7P&lt;BR&gt;
      TM7X&lt;BR&gt;
      -&lt;BR&gt;
      8017SMS&lt;BR&gt;
      -&lt;BR&gt;
      8017SMB&lt;BR&gt;
      8017SMA&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      CT-6W&lt;BR&gt;
      CT-6H&lt;BR&gt;
      CT-6P&lt;BR&gt;
      CT-6R&lt;BR&gt;
      -&lt;BR&gt;
      CT-6V&lt;BR&gt;
      CT-6X&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      8038EKV&lt;BR&gt;
      -&lt;BR&gt;
      8038EKX&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      8038EKP&lt;BR&gt;
      8038EKZ&lt;BR&gt;
      8038EKW&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      3321H&lt;BR&gt;
      3321P&lt;BR&gt;
      3321N&lt;BR&gt;
      1102H&lt;BR&gt;
      1102P&lt;BR&gt;
      1102T&lt;BR&gt;
      RVA0911V304A&lt;BR&gt;
      -&lt;BR&gt;
      RVA0911H413A&lt;BR&gt;
      RVG0707V100A&lt;BR&gt;
      RVA0607V(H)306A&lt;BR&gt;
      RVA1214H213A&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      3104B&lt;BR&gt;
      3104C&lt;BR&gt;
      3104F&lt;BR&gt;
      3104H&lt;BR&gt;
      -&lt;BR&gt;
      3104M&lt;BR&gt;
      3104P&lt;BR&gt;
      3104S&lt;BR&gt;
      3104W&lt;BR&gt;
      3104X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      EVMQ0G&lt;BR&gt;
      EVMQIG&lt;BR&gt;
      EVMQ3G&lt;BR&gt;
      EVMS0G&lt;BR&gt;
      EVMQ0G&lt;BR&gt;
      EVMG0G&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      EVMK4GA00B&lt;BR&gt;
      EVM30GA00B&lt;BR&gt;
      EVMK0GA00B&lt;BR&gt;
      EVM38GA00B&lt;BR&gt;
      EVMB6&lt;BR&gt;
      EVLQ0&lt;BR&gt;
      -&lt;BR&gt;
      EVMMSG&lt;BR&gt;
      EVMMBG&lt;BR&gt;
      EVMMAG&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      EVMMCS&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      EVMM1&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      EVMM0&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      EVMM3&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      62-3-1&lt;BR&gt;
      62-1-2&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      67R&lt;BR&gt;
      -&lt;BR&gt;
      67P&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      67X&lt;BR&gt;
      63V&lt;BR&gt;
      63S&lt;BR&gt;
      63M&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      63H&lt;BR&gt;
      63P&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      63X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      RJ/RJR50&lt;BR&gt;
      RJ/RJR50&lt;BR&gt;
      RJ/RJR50&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
&lt;/TABLE&gt;
&lt;P&gt;&amp;nbsp;&lt;P&gt;
&lt;TABLE BORDER=0 CELLSPACING=1 CELLPADDING=3&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;
      &lt;FONT color="#0000FF" SIZE=4 FACE=ARIAL&gt;&lt;B&gt;SMD TRIM-POT CROSS REFERENCE&lt;/B&gt;&lt;/FONT&gt;
      &lt;P&gt;
      &lt;FONT SIZE=4 FACE=ARIAL&gt;&lt;B&gt;MULTI-TURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BOURNS&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BI&amp;nbsp;TECH&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;DALE-VISHAY&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PHILIPS/MEPCO&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PANASONIC&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;TOCOS&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;AUX/KYOCERA&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      3224G&lt;BR&gt;
      3224J&lt;BR&gt;
      3224W&lt;BR&gt;
      3269P&lt;BR&gt;
      3269W&lt;BR&gt;
      3269X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      44G&lt;BR&gt;
      44J&lt;BR&gt;
      44W&lt;BR&gt;
      84P&lt;BR&gt;
      84W&lt;BR&gt;
      84X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      ST63Z&lt;BR&gt;
      ST63Y&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      ST5P&lt;BR&gt;
      ST5W&lt;BR&gt;
      ST5X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;
      &lt;FONT SIZE=4 FACE=ARIAL&gt;&lt;B&gt;SINGLE TURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BOURNS&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BI&amp;nbsp;TECH&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;DALE-VISHAY&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PHILIPS/MEPCO&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PANASONIC&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;TOCOS&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;AUX/KYOCERA&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      3314G&lt;BR&gt;
      3314J&lt;BR&gt;
      3364A/B&lt;BR&gt;
      3364C/D&lt;BR&gt;
      3364W/X&lt;BR&gt;
      3313G&lt;BR&gt;
      3313J&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      23B&lt;BR&gt;
      23A&lt;BR&gt;
      21X&lt;BR&gt;
      21W&lt;BR&gt;
      -&lt;BR&gt;
      22B&lt;BR&gt;
      22A&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      ST5YL/ST53YL&lt;BR&gt;
      ST5YJ/5T53YJ&lt;BR&gt;
      ST-23A&lt;BR&gt;
      ST-22B&lt;BR&gt;
      ST-22&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      ST-4B&lt;BR&gt;
      ST-4A&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      ST-3B&lt;BR&gt;
      ST-3A&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      EVM-6YS&lt;BR&gt;
      EVM-1E&lt;BR&gt;
      EVM-1G&lt;BR&gt;
      EVM-1D&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      G4B&lt;BR&gt;
      G4A&lt;BR&gt;
      TR04-3S1&lt;BR&gt;
      TRG04-2S1&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      DVR-43A&lt;BR&gt;
      CVR-42C&lt;BR&gt;
      CVR-42A/C&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
&lt;/TABLE&gt;
&lt;P&gt;
&lt;FONT SIZE=4 FACE=ARIAL&gt;&lt;B&gt;ALT =&amp;nbsp;ALTERNATE&lt;/B&gt;&lt;/FONT&gt;
&lt;P&gt;

&amp;nbsp;
&lt;P&gt;
&lt;/td&gt;
&lt;/tr&gt;
&lt;/table&gt;</description>
<packages>
<package name="C1206">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;</description>
</package>
<package name="153CLV-0810">
<description>&lt;b&gt;Aluminum electrolytic capacitors&lt;/b&gt;&lt;p&gt;
SMD (Chip) Long Life Vertical 153 CLV&lt;p&gt;
http://www.bccomponents.com/</description>
</package>
<package name="RTRIM3296W">
<description>&lt;b&gt;Trimm resistor&lt;/b&gt; BOURNS&lt;p&gt;
Source: &lt;a href="http://www.bourns.com/pdfs/3296.pdf"&gt; Data sheet &lt;/a&gt;</description>
</package>
<package name="M1206">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
MELF 0.25 W</description>
</package>
<package name="R1206">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="AudioJack">
<packages>
<package name="CUI_MJ-3502N">
</package>
</packages>
</library>
<library name="diode">
<description>&lt;b&gt;Diodes&lt;/b&gt;&lt;p&gt;
Based on the following sources:
&lt;ul&gt;
&lt;li&gt;Motorola : www.onsemi.com
&lt;li&gt;Fairchild : www.fairchildsemi.com
&lt;li&gt;Philips : www.semiconductors.com
&lt;li&gt;Vishay : www.vishay.de
&lt;/ul&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="DO35-10">
<description>&lt;B&gt;DIODE&lt;/B&gt;&lt;p&gt;
diameter 2 mm, horizontal, grid 10.16 mm</description>
</package>
</packages>
</library>
<library name="2x8_POWER">
<packages>
<package name="CONN_30316-6002HB_3MM">
</package>
</packages>
</library>
<library name="led">
<description>&lt;b&gt;LEDs&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;&lt;br&gt;
Extended by Federico Battaglin &lt;author&gt;&amp;lt;federico.rd@fdpinternational.com&amp;gt;&lt;/author&gt; with DUOLED</description>
<packages>
<package name="LED3MM">
<description>&lt;B&gt;LED&lt;/B&gt;&lt;p&gt;
3 mm, round</description>
</package>
</packages>
</library>
<library name="V3046M 2">
<packages>
<package name="SOIC127P590X140-14N">
<description>14-SOIC, 1.27 mm pitch, 5.90 mm span, 8.60 X 3.85 X 1.40 mm body
&lt;p&gt;14-pin SOIC package with 1.27 mm pitch, 5.90 mm span with body size 8.60 X 3.85 X 1.40 mm&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="switch-dil">
<description>&lt;b&gt;DIL Switches and Code Switches&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="DP-04">
<description>&lt;b&gt;DIL/CODE SWITCH&lt;/b&gt;&lt;p&gt;
distributor Buerklin, 17G570</description>
</package>
</packages>
</library>
<library name="4-1825136-5">
<packages>
<package name="TE_4-1825136-5">
</package>
</packages>
</library>
<library name="transistor">
<description>&lt;b&gt;Transistors&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="SOT23">
<description>&lt;b&gt;SOT-23&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="REF102AU">
<packages>
<package name="SOIC127P599X175-8N">
</package>
</packages>
</library>
<library name="TL072ACD">
<packages>
<package name="SOIC127P599X175-8N">
</package>
</packages>
</library>
<library name="Fairchild_By_element14_Batch_1">
<description>Developed by element14 :&lt;br&gt;
element14 CAD Library consolidation.ulp
at 27/07/2012 14:48:47</description>
<packages>
<package name="SOIC127P600X175-14N">
</package>
</packages>
</library>
<library name="Potentiometer_Trimmers">
<description>&lt;h3&gt; PCBLayout.com - Frequently Used &lt;i&gt;Potentiometers/Trimmers&lt;/i&gt;&lt;/h3&gt;

Visit us at &lt;a href="http://www.PCBLayout.com"&gt;PCBLayout.com&lt;/a&gt; for quick and hassle-free PCB Layout/Manufacturing ordering experience.
&lt;BR&gt;
&lt;BR&gt;
This library has been generated by our experienced pcb layout engineers using current IPC and/or industry standards. We &lt;b&gt;believe&lt;/b&gt; the content to be accurate, complete and current. But, this content is provided as a courtesy and &lt;u&gt;user assumes all risk and responsiblity of it's usage&lt;/u&gt;.
&lt;BR&gt;
&lt;BR&gt;
Feel free to contact us at &lt;a href="mailto:Support@PCBLayout.com"&gt;Support@PCBLayout.com&lt;/a&gt; if you have any questions/concerns regarding any of our content or services.</description>
<packages>
<package name="3310Y-001-104L-ND">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C1" library="rcl" package="C1206" value="1u">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="24"/>
<attribute name="SPICEPREFIX" value="C"/>
<attribute name="VALUE"/>
</element>
<element name="C10" library="rcl" package="C1206" value="100n">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="24"/>
<attribute name="SPICEPREFIX" value="C"/>
<attribute name="VALUE"/>
</element>
<element name="C11" library="rcl" package="C1206" value="100n">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="24"/>
<attribute name="SPICEPREFIX" value="C"/>
<attribute name="VALUE"/>
</element>
<element name="C12" library="rcl" package="C1206" value="100n">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="24"/>
<attribute name="SPICEPREFIX" value="C"/>
<attribute name="VALUE"/>
</element>
<element name="C13" library="rcl" package="C1206" value="100n">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="24"/>
<attribute name="SPICEPREFIX" value="C"/>
<attribute name="VALUE"/>
</element>
<element name="C14" library="rcl" package="C1206" value="100n">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="24"/>
<attribute name="SPICEPREFIX" value="C"/>
<attribute name="VALUE"/>
</element>
<element name="C15" library="rcl" package="C1206" value="100n">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="24"/>
<attribute name="SPICEPREFIX" value="C"/>
<attribute name="VALUE"/>
</element>
<element name="C16" library="rcl" package="C1206" value="100n">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="24"/>
<attribute name="SPICEPREFIX" value="C"/>
<attribute name="VALUE"/>
</element>
<element name="C17" library="rcl" package="153CLV-0810" value="10u">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="3"/>
<attribute name="SPICEPREFIX" value="C"/>
<attribute name="VALUE"/>
</element>
<element name="C18" library="rcl" package="153CLV-0810" value="10u">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="3"/>
<attribute name="SPICEPREFIX" value="C"/>
<attribute name="VALUE"/>
</element>
<element name="C2" library="rcl" package="C1206" value="1u">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="24"/>
<attribute name="SPICEPREFIX" value="C"/>
<attribute name="VALUE"/>
</element>
<element name="C3" library="rcl" package="C1206" value="100p">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="24"/>
<attribute name="SPICEPREFIX" value="C"/>
<attribute name="VALUE"/>
</element>
<element name="C4" library="rcl" package="C1206" value="470p">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="24"/>
<attribute name="SPICEPREFIX" value="C"/>
<attribute name="VALUE"/>
</element>
<element name="C5" library="rcl" package="C1206" value="10n">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="24"/>
<attribute name="SPICEPREFIX" value="C"/>
<attribute name="VALUE"/>
</element>
<element name="C6" library="rcl" package="C1206" value="12p">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="24"/>
<attribute name="SPICEPREFIX" value="C"/>
<attribute name="VALUE"/>
</element>
<element name="C7" library="rcl" package="153CLV-0810" value="100u">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="3"/>
<attribute name="SPICEPREFIX" value="C"/>
<attribute name="VALUE"/>
</element>
<element name="C8" library="rcl" package="153CLV-0810" value="10u">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="3"/>
<attribute name="SPICEPREFIX" value="C"/>
<attribute name="VALUE"/>
</element>
<element name="C9" library="rcl" package="153CLV-0810" value="10u">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="3"/>
<attribute name="SPICEPREFIX" value="C"/>
<attribute name="VALUE"/>
</element>
<element name="CV_INPUT" library="AudioJack" package="CUI_MJ-3502N" value="MJ-3502N">
<attribute name="AVAILABILITY" value="Good"/>
<attribute name="CUI_PURCHASE_URL" value="https://www.cuidevices.com/product/interconnect/connectors/audio-connectors/jacks/mj-3502n?utm_source=snapeda.com&amp;utm_medium=referral&amp;utm_campaign=snapedaBOM"/>
<attribute name="DESCRIPTION" value="3.5 mm, Mono, Right Angle, Through Hole, 2 Conductors, 1 Internal Switch, Audio Jack Connector"/>
<attribute name="MF" value="CUI Devices"/>
<attribute name="MP" value="MJ-3502N"/>
<attribute name="NAME"/>
<attribute name="PACKAGE" value="None"/>
<attribute name="PRICE" value="None"/>
<attribute name="PURCHASE-URL" value="https://pricing.snapeda.com/search/part/MJ-3502N/?ref=eda"/>
<attribute name="VALUE"/>
</element>
<element name="D1" library="diode" package="DO35-10" value="1N4148">
<attribute name="POPULARITY" value="21"/>
<attribute name="VALUE"/>
</element>
<element name="D2" library="diode" package="DO35-10" value="1N4148">
<attribute name="POPULARITY" value="21"/>
<attribute name="VALUE"/>
</element>
<element name="FM" library="AudioJack" package="CUI_MJ-3502N" value="MJ-3502N">
<attribute name="AVAILABILITY" value="Good"/>
<attribute name="CUI_PURCHASE_URL" value="https://www.cuidevices.com/product/interconnect/connectors/audio-connectors/jacks/mj-3502n?utm_source=snapeda.com&amp;utm_medium=referral&amp;utm_campaign=snapedaBOM"/>
<attribute name="DESCRIPTION" value="3.5 mm, Mono, Right Angle, Through Hole, 2 Conductors, 1 Internal Switch, Audio Jack Connector"/>
<attribute name="MF" value="CUI Devices"/>
<attribute name="MP" value="MJ-3502N"/>
<attribute name="NAME"/>
<attribute name="PACKAGE" value="None"/>
<attribute name="PRICE" value="None"/>
<attribute name="PURCHASE-URL" value="https://pricing.snapeda.com/search/part/MJ-3502N/?ref=eda"/>
<attribute name="VALUE"/>
</element>
<element name="J1" library="2x8_POWER" package="CONN_30316-6002HB_3MM" value="30316-6002HB">
<attribute name="BUILT_BY" value="EMA_Cory"/>
<attribute name="COPYRIGHT" value="Copyright (C) 2018 Accelerated Designs. All rights reserved"/>
<attribute name="DATASHEET" value="http://multimedia.3m.com/mws/media/22504O/3mtm-100-in-loprof-hdr-100x-100strt-ra-4-wall-ts0818.pdf"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="30316-6002HB"/>
<attribute name="NAME"/>
<attribute name="SOURCELIBRARY" value="3M_2020-04-20"/>
<attribute name="VALUE"/>
<attribute name="VENDOR" value="3M"/>
</element>
<element name="LED1" library="led" package="LED3MM" value="">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="97"/>
<attribute name="VALUE"/>
</element>
<element name="LED2" library="led" package="LED3MM" value="">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="97"/>
<attribute name="VALUE"/>
</element>
<element name="LM3046" library="V3046M 2" package="SOIC127P590X140-14N" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="OUTPUT" library="AudioJack" package="CUI_MJ-3502N" value="MJ-3502N">
<attribute name="AVAILABILITY" value="Good"/>
<attribute name="CUI_PURCHASE_URL" value="https://www.cuidevices.com/product/interconnect/connectors/audio-connectors/jacks/mj-3502n?utm_source=snapeda.com&amp;utm_medium=referral&amp;utm_campaign=snapedaBOM"/>
<attribute name="DESCRIPTION" value="3.5 mm, Mono, Right Angle, Through Hole, 2 Conductors, 1 Internal Switch, Audio Jack Connector"/>
<attribute name="MF" value="CUI Devices"/>
<attribute name="MP" value="MJ-3502N"/>
<attribute name="NAME"/>
<attribute name="PACKAGE" value="None"/>
<attribute name="PRICE" value="None"/>
<attribute name="PURCHASE-URL" value="https://pricing.snapeda.com/search/part/MJ-3502N/?ref=eda"/>
<attribute name="VALUE"/>
</element>
<element name="R1" library="rcl" package="R1206" value="10k">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="19"/>
<attribute name="SPICEPREFIX" value="R"/>
<attribute name="VALUE"/>
</element>
<element name="R10" library="rcl" package="R1206" value="2k4">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="19"/>
<attribute name="SPICEPREFIX" value="R"/>
<attribute name="VALUE"/>
</element>
<element name="R11" library="rcl" package="RTRIM3296W" value="200">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="3"/>
<attribute name="SPICEMODEL" value="X"/>
<attribute name="SPICEPREFIXL" value="POT"/>
<attribute name="VALUE"/>
</element>
<element name="R12" library="rcl" package="R1206" value="750">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="19"/>
<attribute name="SPICEPREFIX" value="R"/>
<attribute name="VALUE"/>
</element>
<element name="R13" library="rcl" package="R1206" value="1M">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="19"/>
<attribute name="SPICEPREFIX" value="R"/>
<attribute name="VALUE"/>
</element>
<element name="R14" library="rcl" package="R1206" value="56k">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="19"/>
<attribute name="SPICEPREFIX" value="R"/>
<attribute name="VALUE"/>
</element>
<element name="R15" library="rcl" package="RTRIM3296W" value="100k">
<attribute name="NAME"/>
<attribute name="NOTE" value="Linear"/>
<attribute name="POPULARITY" value="3"/>
<attribute name="SPICEMODEL" value="X"/>
<attribute name="SPICEPREFIXL" value="POT"/>
<attribute name="VALUE"/>
</element>
<element name="R16" library="rcl" package="R1206" value="1k">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="19"/>
<attribute name="SPICEPREFIX" value="R"/>
<attribute name="VALUE"/>
</element>
<element name="R17" library="rcl" package="R1206" value="1k">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="19"/>
<attribute name="SPICEPREFIX" value="R"/>
<attribute name="VALUE"/>
</element>
<element name="R18" library="rcl" package="R1206" value="1k">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="19"/>
<attribute name="SPICEPREFIX" value="R"/>
<attribute name="VALUE"/>
</element>
<element name="R19" library="rcl" package="R1206" value="10k">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="19"/>
<attribute name="SPICEPREFIX" value="R"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="rcl" package="R1206" value="10k">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="19"/>
<attribute name="SPICEPREFIX" value="R"/>
<attribute name="VALUE"/>
</element>
<element name="R20" library="rcl" package="M1206" value="1k">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="22"/>
<attribute name="SPICEPREFIX" value="R"/>
<attribute name="VALUE"/>
</element>
<element name="R21" library="rcl" package="R1206" value="10k">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="19"/>
<attribute name="SPICEPREFIX" value="R"/>
<attribute name="VALUE"/>
</element>
<element name="R22" library="rcl" package="R1206" value="220">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="19"/>
<attribute name="SPICEPREFIX" value="R"/>
<attribute name="VALUE"/>
</element>
<element name="R23" library="rcl" package="RTRIM3296W" value="5K">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="3"/>
<attribute name="SPICEMODEL" value="X"/>
<attribute name="SPICEPREFIXL" value="POT"/>
<attribute name="VALUE"/>
</element>
<element name="R24" library="rcl" package="RTRIM3296W" value="10K">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="3"/>
<attribute name="SPICEMODEL" value="X"/>
<attribute name="SPICEPREFIXL" value="POT"/>
<attribute name="VALUE"/>
</element>
<element name="R25" library="rcl" package="R1206" value="20K">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="19"/>
<attribute name="SPICEPREFIX" value="R"/>
<attribute name="VALUE"/>
</element>
<element name="R26" library="rcl" package="R1206" value="10K">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="19"/>
<attribute name="SPICEPREFIX" value="R"/>
<attribute name="VALUE"/>
</element>
<element name="R27" library="rcl" package="R1206" value="1K2">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="19"/>
<attribute name="SPICEPREFIX" value="R"/>
<attribute name="VALUE"/>
</element>
<element name="R28" library="rcl" package="R1206" value="100">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="19"/>
<attribute name="SPICEPREFIX" value="R"/>
<attribute name="VALUE"/>
</element>
<element name="R29" library="rcl" package="R1206" value="6K2">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="19"/>
<attribute name="SPICEPREFIX" value="R"/>
<attribute name="VALUE"/>
</element>
<element name="R3" library="rcl" package="R1206" value="100k">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="19"/>
<attribute name="SPICEPREFIX" value="R"/>
<attribute name="VALUE"/>
</element>
<element name="R30" library="rcl" package="R1206" value="3K3">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="19"/>
<attribute name="SPICEPREFIX" value="R"/>
<attribute name="VALUE"/>
</element>
<element name="R31" library="rcl" package="R1206" value="360">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="19"/>
<attribute name="SPICEPREFIX" value="R"/>
<attribute name="VALUE"/>
</element>
<element name="R32" library="rcl" package="R1206" value="330">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="19"/>
<attribute name="SPICEPREFIX" value="R"/>
<attribute name="VALUE"/>
</element>
<element name="R33" library="rcl" package="RTRIM3296W" value="10k">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="3"/>
<attribute name="SPICEMODEL" value="X"/>
<attribute name="SPICEPREFIXL" value="POT"/>
<attribute name="VALUE"/>
</element>
<element name="R34" library="rcl" package="R1206" value="100">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="19"/>
<attribute name="SPICEPREFIX" value="R"/>
<attribute name="VALUE"/>
</element>
<element name="R35" library="rcl" package="RTRIM3296W" value="10k">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="3"/>
<attribute name="SPICEMODEL" value="X"/>
<attribute name="SPICEPREFIXL" value="POT"/>
<attribute name="VALUE"/>
</element>
<element name="R36" library="rcl" package="R1206" value="240">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="19"/>
<attribute name="SPICEPREFIX" value="R"/>
<attribute name="VALUE"/>
</element>
<element name="R37" library="rcl" package="R1206" value="1k">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="19"/>
<attribute name="SPICEPREFIX" value="R"/>
<attribute name="VALUE"/>
</element>
<element name="R4" library="rcl" package="R1206" value="100k">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="19"/>
<attribute name="SPICEPREFIX" value="R"/>
<attribute name="VALUE"/>
</element>
<element name="R5" library="rcl" package="R1206" value="100k">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="19"/>
<attribute name="SPICEPREFIX" value="R"/>
<attribute name="VALUE"/>
</element>
<element name="R6" library="rcl" package="R1206" value="100k">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="19"/>
<attribute name="SPICEPREFIX" value="R"/>
<attribute name="VALUE"/>
</element>
<element name="R7" library="rcl" package="R1206" value="100k">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="19"/>
<attribute name="SPICEPREFIX" value="R"/>
<attribute name="VALUE"/>
</element>
<element name="R8" library="rcl" package="R1206" value="100k">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="19"/>
<attribute name="SPICEPREFIX" value="R"/>
<attribute name="VALUE"/>
</element>
<element name="R9" library="rcl" package="R1206" value="430k">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="19"/>
<attribute name="SPICEPREFIX" value="R"/>
<attribute name="VALUE"/>
</element>
<element name="S1" library="switch-dil" package="DP-04" value="SETTINGS">
<attribute name="MF" value=""/>
<attribute name="MPN" value="DP04"/>
<attribute name="NAME"/>
<attribute name="OC_FARNELL" value="9471600"/>
<attribute name="OC_NEWARK" value="73J0027"/>
<attribute name="VALUE"/>
</element>
<element name="S2" library="4-1825136-5" package="TE_4-1825136-5" value="4-1825136-5">
<attribute name="COMMENT" value="4-1825136-5"/>
<attribute name="DESCRIPTION" value=" Switch Toggle ON None ON SPDT Long Baton Lever PC Pins 5A 250VAC 28VDC PC Mount with Threads Bulk "/>
<attribute name="DIGI-KEY_PART_NUMBER" value="450-1784-ND"/>
<attribute name="EU_ROHS_COMPLIANCE" value="Compliant with Exemptions"/>
<attribute name="MF" value="TE Connectivity"/>
<attribute name="MP" value="4-1825136-5"/>
<attribute name="NAME"/>
<attribute name="PACKAGE" value="SOIC-8 TE Connectivity"/>
<attribute name="PURCHASE-URL" value="https://pricing.snapeda.com/search/part/4-1825136-5/?ref=eda"/>
</element>
<element name="SYNC" library="AudioJack" package="CUI_MJ-3502N" value="MJ-3502N">
<attribute name="AVAILABILITY" value="Good"/>
<attribute name="CUI_PURCHASE_URL" value="https://www.cuidevices.com/product/interconnect/connectors/audio-connectors/jacks/mj-3502n?utm_source=snapeda.com&amp;utm_medium=referral&amp;utm_campaign=snapedaBOM"/>
<attribute name="DESCRIPTION" value="3.5 mm, Mono, Right Angle, Through Hole, 2 Conductors, 1 Internal Switch, Audio Jack Connector"/>
<attribute name="MF" value="CUI Devices"/>
<attribute name="MP" value="MJ-3502N"/>
<attribute name="NAME"/>
<attribute name="PACKAGE" value="None"/>
<attribute name="PRICE" value="None"/>
<attribute name="PURCHASE-URL" value="https://pricing.snapeda.com/search/part/MJ-3502N/?ref=eda"/>
<attribute name="VALUE"/>
</element>
<element name="T1" library="transistor" package="SOT23" value="BC850">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="0"/>
<attribute name="VALUE"/>
</element>
<element name="T2" library="transistor" package="SOT23" value="BC850">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="0"/>
<attribute name="VALUE"/>
</element>
<element name="T3" library="transistor" package="SOT23" value="BC850">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="0"/>
<attribute name="VALUE"/>
</element>
<element name="T4" library="transistor" package="SOT23" value="BC850">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="0"/>
<attribute name="VALUE"/>
</element>
<element name="T5" library="transistor" package="SOT23" value="BC850">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="0"/>
<attribute name="VALUE"/>
</element>
<element name="U1" library="REF102AU" package="SOIC127P599X175-8N" value="REF102AU">
<attribute name="DESCRIPTION" value=" 2.5-ppm/C drift, 10-V precision voltage reference 8-SOIC "/>
<attribute name="DIGI-KEY_PART_NUMBER" value="296-41381-2-ND"/>
<attribute name="MF" value="Texas Instruments"/>
<attribute name="MP" value="REF102AU"/>
<attribute name="NAME"/>
<attribute name="PACKAGE" value="SOIC-8 Texas Instruments"/>
<attribute name="PURCHASE-URL" value="https://pricing.snapeda.com/search/part/REF102AU/?ref=eda"/>
<attribute name="VALUE"/>
</element>
<element name="U2" library="TL072ACD" package="SOIC127P599X175-8N" value="TL072ACD">
<attribute name="AVAILABILITY" value="Good"/>
<attribute name="DESCRIPTION" value=" Dual low-noise JFET-input improved offset operational amplifier 8-SOIC 0 to 70 "/>
<attribute name="MF" value="Texas Instruments"/>
<attribute name="MP" value="TL072ACD"/>
<attribute name="NAME"/>
<attribute name="PACKAGE" value="SOIC-8 Texas Instruments"/>
<attribute name="PRICE" value="None"/>
<attribute name="PURCHASE-URL" value="https://pricing.snapeda.com/search/part/TL072ACD/?ref=eda"/>
<attribute name="VALUE"/>
</element>
<element name="U3" library="TL072ACD" package="SOIC127P599X175-8N" value="TL072ACD">
<attribute name="AVAILABILITY" value="Good"/>
<attribute name="DESCRIPTION" value=" Dual low-noise JFET-input improved offset operational amplifier 8-SOIC 0 to 70 "/>
<attribute name="MF" value="Texas Instruments"/>
<attribute name="MP" value="TL072ACD"/>
<attribute name="NAME"/>
<attribute name="PACKAGE" value="SOIC-8 Texas Instruments"/>
<attribute name="PRICE" value="None"/>
<attribute name="PURCHASE-URL" value="https://pricing.snapeda.com/search/part/TL072ACD/?ref=eda"/>
<attribute name="VALUE"/>
</element>
<element name="U4" library="TL072ACD" package="SOIC127P599X175-8N" value="TL072ACD">
<attribute name="AVAILABILITY" value="Good"/>
<attribute name="DESCRIPTION" value=" Dual low-noise JFET-input improved offset operational amplifier 8-SOIC 0 to 70 "/>
<attribute name="MF" value="Texas Instruments"/>
<attribute name="MP" value="TL072ACD"/>
<attribute name="NAME"/>
<attribute name="PACKAGE" value="SOIC-8 Texas Instruments"/>
<attribute name="PRICE" value="None"/>
<attribute name="PURCHASE-URL" value="https://pricing.snapeda.com/search/part/TL072ACD/?ref=eda"/>
<attribute name="VALUE"/>
</element>
<element name="U5" library="Fairchild_By_element14_Batch_1" package="SOIC127P600X175-14N" value="CD4093BCM">
<attribute name="MPN" value="CD4093BCM"/>
<attribute name="NAME"/>
<attribute name="OC_FARNELL" value="1014068"/>
<attribute name="OC_NEWARK" value="78K5876"/>
<attribute name="PACKAGE" value="SOIC-14"/>
<attribute name="SUPPLIER" value="Fairchild"/>
<attribute name="VALUE"/>
</element>
<element name="U6" library="TL072ACD" package="SOIC127P599X175-8N" value="TL072ACD">
<attribute name="AVAILABILITY" value="Good"/>
<attribute name="DESCRIPTION" value=" Dual low-noise JFET-input improved offset operational amplifier 8-SOIC 0 to 70 "/>
<attribute name="MF" value="Texas Instruments"/>
<attribute name="MP" value="TL072ACD"/>
<attribute name="NAME"/>
<attribute name="PACKAGE" value="SOIC-8 Texas Instruments"/>
<attribute name="PRICE" value="None"/>
<attribute name="PURCHASE-URL" value="https://pricing.snapeda.com/search/part/TL072ACD/?ref=eda"/>
<attribute name="VALUE"/>
</element>
<element name="VR1" library="Potentiometer_Trimmers" package="3310Y-001-104L-ND" value="3310Y-001-104L">
<attribute name="CREATED_BY" value=" PCBLayout.com"/>
<attribute name="DIGIKEY_PARTNO" value="3310Y-001-104L-ND"/>
<attribute name="MANUFACTURER" value="Bourns Inc."/>
<attribute name="MPN" value="3310Y-001-104L"/>
<attribute name="NAME"/>
<attribute name="RESITANCE" value="100k"/>
</element>
<element name="VR2" library="Potentiometer_Trimmers" package="3310Y-001-104L-ND" value="3310Y-001-104L">
<attribute name="CREATED_BY" value=" PCBLayout.com"/>
<attribute name="DIGIKEY_PARTNO" value="3310Y-001-104L-ND"/>
<attribute name="MANUFACTURER" value="Bourns Inc."/>
<attribute name="MPN" value="3310Y-001-104L"/>
<attribute name="NAME"/>
<attribute name="RESISTANCE" value="100k"/>
</element>
<element name="VR3" library="Potentiometer_Trimmers" package="3310Y-001-104L-ND" value="3310Y-001-104L">
<attribute name="CREATED_BY" value=" PCBLayout.com"/>
<attribute name="DIGIKEY_PARTNO" value="3310Y-001-104L-ND"/>
<attribute name="MANUFACTURER" value="Bourns Inc."/>
<attribute name="MPN" value="3310Y-001-104L"/>
<attribute name="NAME"/>
<attribute name="RESISTANCE" value="10k"/>
</element>
</elements>
<signals>
<signal name="VCC+">
<contactref element="U6" pad="8"/>
</signal>
<signal name="VCC-">
<contactref element="U6" pad="4"/>
</signal>
<signal name="+10V">
<contactref element="U1" pad="6"/>
<contactref element="R1" pad="1"/>
<contactref element="R7" pad="2"/>
<contactref element="R13" pad="1"/>
<contactref element="R25" pad="2"/>
<contactref element="R26" pad="2"/>
</signal>
<signal name="N$1">
<contactref element="R1" pad="2"/>
<contactref element="U3" pad="2"/>
</signal>
<signal name="-10V">
<contactref element="U3" pad="1"/>
<contactref element="R2" pad="2"/>
<contactref element="R6" pad="1"/>
<contactref element="VR2" pad="1"/>
</signal>
<signal name="N$2">
<contactref element="U3" pad="3"/>
<contactref element="R2" pad="1"/>
</signal>
<signal name="+12V">
<contactref element="U1" pad="2"/>
<contactref element="C1" pad="2"/>
<contactref element="U3" pad="8"/>
<contactref element="J1" pad="9"/>
<contactref element="J1" pad="10"/>
<contactref element="U4" pad="8"/>
<contactref element="U2" pad="8"/>
<contactref element="T5" pad="3"/>
<contactref element="R35" pad="1"/>
<contactref element="C17" pad="+"/>
<contactref element="C13" pad="1"/>
<contactref element="C12" pad="1"/>
<contactref element="C11" pad="1"/>
<contactref element="C8" pad="+"/>
</signal>
<signal name="GND">
<contactref element="C1" pad="1"/>
<contactref element="U1" pad="4"/>
<contactref element="C2" pad="2"/>
<contactref element="J1" pad="3"/>
<contactref element="J1" pad="5"/>
<contactref element="J1" pad="7"/>
<contactref element="J1" pad="4"/>
<contactref element="J1" pad="6"/>
<contactref element="J1" pad="8"/>
<contactref element="CV_INPUT" pad="1"/>
<contactref element="FM" pad="1"/>
<contactref element="VR1" pad="3"/>
<contactref element="VR2" pad="3"/>
<contactref element="R12" pad="2"/>
<contactref element="U4" pad="5"/>
<contactref element="LM3046" pad="4"/>
<contactref element="SYNC" pad="1"/>
<contactref element="R15" pad="3"/>
<contactref element="T1" pad="2"/>
<contactref element="U5" pad="7"/>
<contactref element="D1" pad="A"/>
<contactref element="T2" pad="2"/>
<contactref element="T3" pad="2"/>
<contactref element="U5" pad="13"/>
<contactref element="U5" pad="12"/>
<contactref element="U5" pad="9"/>
<contactref element="U5" pad="8"/>
<contactref element="U5" pad="6"/>
<contactref element="U5" pad="5"/>
<contactref element="R27" pad="1"/>
<contactref element="LM3046" pad="7"/>
<contactref element="R30" pad="2"/>
<contactref element="R32" pad="2"/>
<contactref element="R31" pad="2"/>
<contactref element="R35" pad="3"/>
<contactref element="OUTPUT" pad="1"/>
<contactref element="LED2" pad="K"/>
<contactref element="LED1" pad="A"/>
<contactref element="U3" pad="5"/>
<contactref element="U3" pad="6"/>
<contactref element="C7" pad="-"/>
<contactref element="C10" pad="2"/>
<contactref element="C17" pad="-"/>
<contactref element="C18" pad="+"/>
<contactref element="C8" pad="-"/>
<contactref element="C9" pad="+"/>
<contactref element="C11" pad="2"/>
<contactref element="C14" pad="1"/>
<contactref element="C12" pad="2"/>
<contactref element="C15" pad="1"/>
<contactref element="C13" pad="2"/>
<contactref element="C16" pad="1"/>
</signal>
<signal name="N$4">
<contactref element="U1" pad="8"/>
<contactref element="C2" pad="1"/>
</signal>
<signal name="-12V">
<contactref element="J1" pad="1"/>
<contactref element="U3" pad="4"/>
<contactref element="J1" pad="2"/>
<contactref element="U4" pad="4"/>
<contactref element="U2" pad="4"/>
<contactref element="C18" pad="-"/>
<contactref element="C16" pad="2"/>
<contactref element="C15" pad="2"/>
<contactref element="C14" pad="2"/>
<contactref element="C9" pad="-"/>
</signal>
<signal name="+5V">
<contactref element="J1" pad="11"/>
<contactref element="J1" pad="12"/>
<contactref element="R17" pad="2"/>
<contactref element="D2" pad="C"/>
<contactref element="R19" pad="2"/>
<contactref element="R21" pad="2"/>
<contactref element="U5" pad="14"/>
<contactref element="T4" pad="3"/>
<contactref element="C4" pad="1"/>
<contactref element="C7" pad="+"/>
<contactref element="C10" pad="1"/>
</signal>
<signal name="CV">
<contactref element="J1" pad="13"/>
<contactref element="J1" pad="14"/>
<contactref element="S1" pad="8"/>
<contactref element="S1" pad="7"/>
</signal>
<signal name="GATE">
<contactref element="J1" pad="15"/>
<contactref element="J1" pad="16"/>
</signal>
<signal name="CV_ON_JACK">
<contactref element="S1" pad="1"/>
<contactref element="CV_INPUT" pad="3"/>
</signal>
<signal name="CV_ON_SWITCH">
<contactref element="S1" pad="2"/>
<contactref element="R4" pad="1"/>
</signal>
<signal name="CV_INPUT">
<contactref element="CV_INPUT" pad="2"/>
<contactref element="R3" pad="1"/>
</signal>
<signal name="N$5">
<contactref element="R3" pad="2"/>
<contactref element="S2" pad="1"/>
</signal>
<signal name="N$6">
<contactref element="R4" pad="2"/>
<contactref element="S2" pad="3"/>
</signal>
<signal name="FM_SIGNAL">
<contactref element="FM" pad="3"/>
<contactref element="FM" pad="2"/>
<contactref element="VR1" pad="1"/>
</signal>
<signal name="CONDITIONED_FM">
<contactref element="VR1" pad="2"/>
<contactref element="R5" pad="1"/>
</signal>
<signal name="OSC_INPUT">
<contactref element="R5" pad="2"/>
<contactref element="S2" pad="2"/>
<contactref element="R9" pad="2"/>
<contactref element="R8" pad="2"/>
<contactref element="U4" pad="2"/>
</signal>
<signal name="N$3">
<contactref element="R6" pad="2"/>
<contactref element="VR3" pad="1"/>
</signal>
<signal name="N$7">
<contactref element="VR3" pad="3"/>
<contactref element="R7" pad="1"/>
</signal>
<signal name="N$8">
<contactref element="VR3" pad="2"/>
<contactref element="R9" pad="1"/>
</signal>
<signal name="N$9">
<contactref element="VR2" pad="2"/>
<contactref element="R8" pad="1"/>
</signal>
<signal name="N$10">
<contactref element="R10" pad="2"/>
<contactref element="R11" pad="1"/>
<contactref element="U4" pad="1"/>
</signal>
<signal name="N$11">
<contactref element="R10" pad="1"/>
<contactref element="U4" pad="3"/>
</signal>
<signal name="N$12">
<contactref element="R11" pad="3"/>
<contactref element="R12" pad="1"/>
</signal>
<signal name="N$14">
<contactref element="R11" pad="2"/>
<contactref element="LM3046" pad="2"/>
</signal>
<signal name="VI_FEEDBACK">
<contactref element="R13" pad="2"/>
<contactref element="C3" pad="1"/>
<contactref element="U4" pad="6"/>
<contactref element="LM3046" pad="1"/>
</signal>
<signal name="N$13">
<contactref element="R14" pad="2"/>
<contactref element="LM3046" pad="3"/>
</signal>
<signal name="N$16">
<contactref element="R14" pad="1"/>
<contactref element="C3" pad="2"/>
<contactref element="U4" pad="7"/>
</signal>
<signal name="SYNCH_JACK">
<contactref element="SYNC" pad="2"/>
<contactref element="R15" pad="1"/>
<contactref element="SYNC" pad="3"/>
</signal>
<signal name="SCALED_SYNC">
<contactref element="R16" pad="1"/>
<contactref element="R15" pad="2"/>
</signal>
<signal name="SYNC_TO_TRANSISTOR">
<contactref element="R16" pad="2"/>
<contactref element="T1" pad="1"/>
</signal>
<signal name="SYNC_IN">
<contactref element="T1" pad="3"/>
<contactref element="R17" pad="1"/>
<contactref element="U5" pad="2"/>
</signal>
<signal name="WAVE_GEN_OUT">
<contactref element="U2" pad="2"/>
<contactref element="U2" pad="1"/>
<contactref element="R18" pad="1"/>
</signal>
<signal name="WAVE_GEN_STAGE_1">
<contactref element="R18" pad="2"/>
<contactref element="T2" pad="1"/>
<contactref element="D1" pad="C"/>
<contactref element="D2" pad="A"/>
</signal>
<signal name="WAVE_GEN_STAGE_2A">
<contactref element="T2" pad="3"/>
<contactref element="R19" pad="1"/>
<contactref element="R20" pad="2"/>
</signal>
<signal name="WAVE_GEN_STAGE_2B">
<contactref element="R20" pad="1"/>
<contactref element="T3" pad="1"/>
</signal>
<signal name="WAVE_GEN_STAGE_C">
<contactref element="T3" pad="3"/>
<contactref element="R21" pad="1"/>
<contactref element="U5" pad="1"/>
</signal>
<signal name="LOGIC_GATE_OUT">
<contactref element="U5" pad="3"/>
<contactref element="R22" pad="1"/>
</signal>
<signal name="CONDITIONED_LOGIC_GATE_OUT">
<contactref element="R22" pad="2"/>
<contactref element="T4" pad="1"/>
</signal>
<signal name="RAW_WAVE_OUT">
<contactref element="T4" pad="2"/>
<contactref element="C4" pad="2"/>
<contactref element="R23" pad="3"/>
<contactref element="R23" pad="2"/>
</signal>
<signal name="WAVE_OUT">
<contactref element="LM3046" pad="5"/>
<contactref element="R23" pad="1"/>
<contactref element="U2" pad="3"/>
<contactref element="U6" pad="3"/>
</signal>
<signal name="HEAT+">
<contactref element="R26" pad="1"/>
<contactref element="LM3046" pad="8"/>
<contactref element="LM3046" pad="6"/>
</signal>
<signal name="HEAT-">
<contactref element="R24" pad="2"/>
<contactref element="C5" pad="2"/>
</signal>
<signal name="HEAT_OUT">
<contactref element="U2" pad="7"/>
<contactref element="C5" pad="1"/>
<contactref element="R28" pad="1"/>
</signal>
<signal name="N$17">
<contactref element="R25" pad="1"/>
<contactref element="R24" pad="3"/>
</signal>
<signal name="N$18">
<contactref element="R27" pad="2"/>
<contactref element="R24" pad="1"/>
</signal>
<signal name="HEAT_CTRL">
<contactref element="R28" pad="2"/>
<contactref element="T5" pad="1"/>
</signal>
<signal name="HEAT">
<contactref element="T5" pad="2"/>
<contactref element="R29" pad="2"/>
<contactref element="LM3046" pad="14"/>
<contactref element="LM3046" pad="11"/>
</signal>
<signal name="SOME_KINDA_HEAT_BRIDGE">
<contactref element="LM3046" pad="12"/>
<contactref element="LM3046" pad="9"/>
<contactref element="R29" pad="1"/>
<contactref element="R30" pad="1"/>
</signal>
<signal name="N$15">
<contactref element="LM3046" pad="13"/>
<contactref element="R32" pad="1"/>
</signal>
<signal name="N$19">
<contactref element="LM3046" pad="10"/>
<contactref element="R31" pad="1"/>
</signal>
<signal name="OUTPUT_GAIN/SCALE">
<contactref element="C6" pad="1"/>
<contactref element="R33" pad="1"/>
<contactref element="R34" pad="1"/>
<contactref element="U6" pad="2"/>
</signal>
<signal name="OUTPUT_SCALE">
<contactref element="R34" pad="2"/>
<contactref element="R35" pad="2"/>
</signal>
<signal name="BUFFERED_OUTPUT">
<contactref element="C6" pad="2"/>
<contactref element="R33" pad="2"/>
<contactref element="R33" pad="3"/>
<contactref element="U6" pad="1"/>
<contactref element="R36" pad="1"/>
<contactref element="U6" pad="5"/>
</signal>
<signal name="N$22">
<contactref element="R36" pad="2"/>
<contactref element="OUTPUT" pad="2"/>
<contactref element="OUTPUT" pad="3"/>
</signal>
<signal name="LED_FEEDBACK">
<contactref element="U6" pad="7"/>
<contactref element="U6" pad="6"/>
<contactref element="R37" pad="2"/>
</signal>
<signal name="LED_DRIVE">
<contactref element="R37" pad="1"/>
<contactref element="LED2" pad="A"/>
<contactref element="LED1" pad="K"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
